関連トピック

# サンプル RIPng ルーティング構成ファイル

Fireware XTM で動的ルーティング プロトコルのいずれかを使用するには、選択するルーティング デーモンの 構成ファイアウォールをコピーして貼り付ける必要があります。このトピックには、RIP ルーティング デーモン用のサンプル構成ファイルが含まれます 。この構成ファイルを独自の構成ファイルのベースとして使用する場合、メモ帳またはワードパッドなどのアプリケーションでテキストをコピーし、名前を付けて保存します。業務の要件に合わせてパラメータを編集することができます。

任意コマンドへのコメントは「!」の字を使って追加します。コマンドを有効にするには、「!」を削除し、必要に応じて変数を変更します。

!! SECTION 1: Configure global RIPng daemon properties.
!! Enable RIPng daemon. Must be enabled for all RIPng configurations.
! router ripng

!! SECTION 2: Configure interfaces and networks.
! Enable RIPng on interface(eth0).
! network eth0
! ! Enable RIPng on network (2000::/64)
! network 2000::/64
! ! Set RIPng to receive-only on interface (eth2).
! passive-interface eth2

!! SECTION 3: Redistribute RIPng routes to peers and inject OSPFv3 or BGP routes to RIPng routing table.
!! Share route of last resort (default route) from kernel routing table with RIPng peers.
! default-information originate
!! Redistribute firewall static routes to RIPng peers.
! redistribute static
!! Set route maps (MAPNAME) to restrict route redistribution in Section 4.
! Redistribute routes from all interfaces to RIPng peers or with a route map filter (MAPNAME).
! redistribute connected
! redistribute connected route-map MAPNAME
!! Redistribute routes from OSPFv3 to RIPng or with a route map filter (MAPNAME).
! redistribute ospf6
! redistribute ospf6 route-map MAPNAME
!! Redistribute routes from BGP to RIPng or with a route map filter (MAPNAME).
! redistribute bgp
! redistribute bgp route-map MAPNAME

!! SECTION 4: Configure route redistribution filters with route maps and access lists.
!!Filter networks in incoming routing updates
! distribute-list LISTNAME in
!! Create an ipv6 access list to only allow network 3000::/64.
! ipv6 access-list LISTNAME permit 3000::/64
! ipv6 access-list LISTNAME deny any
!! Create a route map with name MAPNAME and allow with a priority of 10.
! route-map MAPNAME permit 10
! match interface eth1

#### 関連情報

ルーティング情報プロトコル（RIP および RIPng）について

RIPng コマンド

RIPng を使用して IPv6 ルーティングを構成する

フィードバックの送信 • サポートのリクエスト • 全製品ドキュメント • 技術検索